**ANNEX I: Offer to Supply Goods Compliant with Technical Specifications**

*We, the undersigned, hereby offer to supply the items listed below in conformity with the specification and requirements of ANRD as per “Bid Request” with the subject “Offer for Procurement of Equipment for Medicinal Herb Processing” for the non-governmental organization Albanian Network for Rural*

*in the frame of the project ‘Support the economic and social empowerment of rural women in the municipalities of Elbasan, Gramsh and Kolonjë’.*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item No.** | **Description** | **Technical Specification** | **Offered Product** | **Comments** |
|  | **Mill: for herb milling and powdering** | 1. **Non-heating milling**: Use sharp blades or knives to cut the material cleanly without heating it.  2. **Material cushioning**: The mill must be able to grind dry plant material with a moisture content not exceeding 14% without fibrillating it.  3. **Size range**: It should be able to grind material from 0.2 mm up to 2 cm, starting from material initially 20-30 cm long.  4. **Hourly capacity**: The capacity should be between 10 and 50 kg per hour of incoming material.  5. **Fine dust suction system**: It must be suitable for the application of a suction system for fine dust generated during milling (do not include the system in the offer).  Technical specifications:   * + Use of sharp blades or knives to cut the material.   + Ability to adjust the grind size.   + Ability to integrate a dust suction system.   Hygienic design for easy cleaning and maintenance. |  |  |
|  | **Low-Temperature Treatment Chamber to free herbs from insects.** | 1. **Insulated chamber**: The chamber must be insulated and sealed to maintain the internal temperature.  2. **Capacity**: 20 – 30 kg of dried product per 24 hours.  3. **Refrigeration unit**: An appropriately sized refrigeration unit to achieve temperatures of -25°C in approximately 180 minutes.  4. **Wall materials**: Walls can be made of plastic or metal with hygienic and anti-frost surfaces.  5. **Shelves**: Shelves made of metal mesh or plastic, capable of supporting herbs weight  Technical specifications:   * + Temperature control system.   + Door with access hatches.   + Solid and sturdy construction.   + Safety system to ensure product integrity. |  |  |
|  | **Semi-Automatic Weighing Filling Machine for Small Bag Powder** | * Equipment material: stainless steel * Voltage: 220V * Hopper capacity: minimum of 5kg * Filling Range: 2 gr – 99 gr * Filling Speed: 10-25 times/min, 600-1000 bags/hour (Depending on materials and different weight size.) * Filling Accuracy: ±0-0.2g (Depending on material) |  |  |

|  |  |
| --- | --- |
|  | * *Readily available in stock – delivery should occur immediately after placing the purchase order.* * *If not available in stock, ANRD allows for a delivery period of up to two months after the contract signature.* |

Supplier Name

Name and Title of Supplier Representative

Signature Date